Apache HTTP Server Version 2.5

Apache > HTTP Server > Documentation > Version 2.5 > Modules

# Apache Module mod_dialup

Description: | Send static content at a bandwidth rate limit, defined by the various old modem standards
Status: | Experimental
Module Identifier: | dialup_module
Source File: | mod_dialup.c

### Summary

It is a module that sends static content at a bandwidth rate limit, defined by the various old modem standards. So, you can browse your site with a 56k V.92 modem, by adding something like this:

    <Location "/mysite">
        ModemStandard "V.92"
    </Location>

Previously to do bandwidth rate limiting modules would have to block an entire thread, for each client, and insert sleeps to slow the bandwidth down. Using the new suspend feature, a handler can get callback N milliseconds in the future, and it will be invoked by the Event MPM on a different thread, once the timer hits. From there the handler can continue to send data to the client.

### Directives

### Bugfix checklist

- httpd changelog
- Known issues
- Report a bug

## ModemStandard Directive ¶

Description: | Modem standard to simulate
Syntax: | `ModemStandard V.21|V.26bis|V.32|V.34|V.92`
Context: | directory
Status: | Experimental
Module: | mod_dialup

Specify what modem standard you wish to simulate.

    <Location "/mysite">
        ModemStandard "V.26bis"
    </Location>